## LED PAR LIGHT

CATEGORIA:

CENICAS

***CÓDIGO:***

SPL LED P 750

***ESPECIFICAÇÃO:***

Feature:  
1.Par light with 7pcs 50W Dual white LED  
2.Beam angle 25°  
3.Various built-in shows

**POWER**

Input voltage: AC100-240V 50/60Hz

Power consumption: 300W

**FIXTURE**

IP rating: IP20

Cooling method: fan cooling

Max ambient temp: 45℃

Case color: black

**LED**

LED type:7\*50W dual white LED(3000K+6000K)

Average lifespan: 50,000 hours

**CONTROL**

DMX channel: 6/14/18 DMX channels

DMX connector:3-pin XLR input/output

Power connector: IEC power input

Control mode: DMX/master-slave/sound/auto/RDM

Display: LED display with 4 push buttons

Various built-in shows controlled by DMX or menu

**COLOR EFFECT**

Color: 3000K-6000K white mixing

Electronic dimming: 0-100%

Strobe: 1-25Hz

Beam angle: 25˚

**DIMENSION**

Product dimension: 29\*24\*29.5cm

N. W: 3.6 KG

SITE DO PRODUTO:

<http://www.sparklaser.com/en/products/226.html>