## IP65 6 WAY BLINDER JARAG

CATEGORIA:

EFEITOS

***CÓDIGO:***

600 IP

***INFORMAÇÕES:***

6pcs 100W amber COB LED with beam angle 3.5˚   
6 LED inner atmostphere rings + 6 LED outer rings  
IP65 for outdoor use and flicker free operation  
Easy connection at 4 sides to make light wall  
Beam + strobe + wash effect

**POWER**

Input voltage: AC100-240V 50/60Hz

Power consumption: 600W

**FIXTURE**

IP rating: IP65

Cooling method:fan cooling

Max ambient temp: 45℃

Case color: black

**LED**

Blinder LED:6pcs 100W amber COB LED, 2300K

Atmostphere LED: 6x6pcs 1W SMD3535 RGB 3in1 LED

Outer ring LED: 6x32pcs 0.2W SMD5050 RGB 3in1 LED

Average lifespan: 50,000 hours

**CONTROL**

DMX channel: 22/108 channels

DMX connector: IP65 3-Pin XLR input/output with cable

Power connector: IP65 PowerCon input/output with cable

Control mode: DMX/auto/master-slave/RDM

Display: LED display with 4 push buttons

1 LED inner atmostphere ring and 1 LED outer ring around a COB LED

Flicker free operation

Single COB LED control

Various built-in showprograms for LED rings

Temperature control for fan speed and LED brightness

4 silent fans working when over 60℃

Easy connection at 4 sides to make a light wall

**COLOR EFFECT**

Color: 2300K amber and RGB color mixing

Electronic Dimming: 0-100% linear

Strobe: 1-25Hz

Beam angle: 3.5˚

Lux at 5m for 1pc 100W LED: 57000LUX

**DIMENSION**

Product dimension: 560\*271\*443mm

N.W:  20.5KG

SITE DO PRODUTO:

http://www.sparklaser.com/en/products/244.html