## Fat beam laser bar

CATEGORIA:

LASER

***CÓDIGO:***

SPL RGB 5007

***INFORMAÇÕES:***

6pcs fat beam laser diodes   
single laser diode control  
semi-conduct laser diode with stable performance and longe liftspan  
sweeping fat beam with Tilt 90° and Pan 240° to make a great and cost effective beam show,  
applicable for disco, club, KTV, pub, Bar etc

**Specification:**

Power supply:AC 100-240V 50/60Hz

Power consumption:90W

Total Laser power:3W red laser

Laser power/wavelength:6pcs 500mW 638nm  red

Laser safety:class 3B

Pan :240°

Tilt  :90°

Control mode:DMX/Auto/Sound/Master-slave

DMX channel:9/19-1/19-2CH

Display:LED display with 4 buttons

Other features:

semi-conduct laser diode with long lifespan and stable performance,

3pin DMX input/output ,Power Con input/output，

laser beam size: 3.5cm at 3m distance, single laser control

IP rating:IP20

N.W.(KG):12.9KG

G.W.(KG):15.1KG

Product dimension:1000\*129\*230mm

Carton size:124\*46\*33cm(2pcs/carton, G.W:34.2KG)

SITE DO PRODUTO:

http://www.sparklaser.com/en/products/129.html