## IP65 LED Wash light bar

CATEGORIA:

RIBALTA

***CÓDIGO:***

SPL LED 1810 IP

***INFORMAÇÕES:***

IP65  
LED:18x10W 6in1 LED  
Control mode: DMX/auto/master-slave/RDM  
Beam angle: 15˚

**POWER**

Input voltage: AC100-240V 50/60Hz

Power consumption: 133W

**FIXTURE**

IP rating: IP65

Cooling method:Aluminum alloy heat dissipation

Max ambient temp: 45℃

Case color: black

**LED**

LED:18x10W 6in1 LED

Average lifespan: 50,000 hours

**CONTROL**

DMX channel: 12/110 channels

DMX connector: IP65 3-Pin XLR input/output with cable

Power connector: IP65 PowerCon input/output with cable

Control mode: DMX/auto/master-slave/RDM

Display: LED display with 4 push buttons

**COLOR EFFECT**

Color: RGBWYP 6in1 LED

Electronic Dimming: 0-100% linear

Strobe: 1-25Hz

Beam angle: 15˚

**DIMENSION**

Product dimension: 101\*14\*19cm

N. W.:  6.4KG

SITE DO PRODUTO:

<http://www.sparklaser.com/en/products/318.html>