## IP65 LED RIBALTA

## 

CATEGORIA:

RIBALTA

***CÓDIGO:***

RIBALTA 3000 IP

***INFORMAÇÕES:***

1024pcs LED with 36 segments   
IP65 for outdoor use and flicker free operation  
Silent fan with temperature control  
Blinder+strobe + wash effect

**POWER**

Input voltage: AC100-240V 50/60Hz

Power consumption: 500W

**FIXTURE**

IP RATING: IP65

Cooling method:fan cooling

Max ambient temp: 45℃

Case color: black

**LED**

LED 1: 256pcs 1W SMD3535 white LED, 7000K

LED 2: 768pcs 0.5W SMD5050 RGB Tri LED

Average lifespan: 50,000 hours

**CONTROL**

DMX channel: 14/58channels

DMX connector: IP65 3-Pin XLR input/output with cable

Power connector: IP65 PowerCon input/output with cable

Control mode: DMX/auto/master-slave/RDM

Display: LED display with 4 push buttons

16 segments for white LED

32 segments for RGB LED

Flicker free operation

Various built-in showprograms

Temperature control for fan speed and LED brightness

2 silent fans working when over 60℃

**COLOR EFFECT**

Color: white and RGB color mixing

Electronic Dimming: 0-100% linear

Strobe: 1-25Hz

Beam angle: 120˚

**DIMENSION**

Product dimension: 980x105x154mm

N.W:  9.6KG

SITE DO PRODUTO:

http://www.sparklaser.com/en/products/308.html