280 BEAM MOVING HEAD

BEAM 280

CATEGORIA:

BEAM

***CÓDIGO:***

SPL MH 280

***INFORMAÇÕES:***

Original Philip 280W lamp  
215,000lux at 10m & beam angle 2°  
Precise and fast Pan/Tilt movement   
Motorized focus,frost filter,split color  
1 gobo wheel+1 color wheel + 2 prisms overlay+1 rainbow wheel

**POWER**

Input voltage: AC100-240V 50/60Hz

Power consumption: 380W

Fuse：6.3A/250V，￠5\*20

**FIXTURE**

IP rating：IP20

Cooling method: fan cool

Max ambient temp: 45℃

Case color: black

**LAMP**

Lamp: Original Philip 280W lamp

Color Temp: 8000K

Average lifespan: 2,000 hours

**CONTROL**

DMX channel: 16CH

DMX connector: 3Pin XLR input/output

Power connector: PowerCon input

Control mode: DMX/master-slave/auto/sound

Pan: 540º16bits, Tilt: 270º16bits

Precise and fast Pan/Tilt movements

Motorized focus, frost, split color and rainbow effect

3-phase motor for Pan/Tilt, automatic position correction

Static gobo wheel: 14gobos plus open

Static color wheel: 13colors plus open

1pc rainbow effect wheel

Prism 1: 8-facet +16-facet rotating, prism 2: 16-facet rotating

Prism overlay and full color LCD display with 5 buttons

With RMD function and software upload via DMX cable

**COLOR EFFECT**

Color: 13 colors+open, split color, rainbow

Beam angle: 2°

Dimming: 0-100%

Strobe: 0-25Hz

Lux : 215,000Lux @ 10m

**DIMENSION**

Product dimension: 34x25.5x51.5cm

N.W: 14.8KG

Outer carton size: 44x41x54cm

G.W.: 17KG(1pc/carton)

SITE DO PRODUTO:

http://www.sparklaser.com/en/products/120.html