380 BEAM MOVING HEAD IP

CATEGORIA:

BEAM

***CÓDIGO:***

SPL MH 380 IP

380 A

***INFORMAÇÕES:***

380W lamp with 2ºbeam angle and 200000LUX at 15m  
 Motorized focus, frost, split color, rainbow effect  
2 prisms+1 static gobo wheel+1 static color wheel+1 rainbow effect wheel  
Auto high temperature protection for lamp

**POWER**

Input power: AC100-240V

Power frequency: 50/60Hz

Power: 500W

**FIXTURE**

IP rating: IP55

Cooling method: air cooling

Maximum ambient temperature: 45℃

Case color: black

**LAMP**

lamp: 380W discharge lamp

Color temperature: 8000K

Average lamp lifespan: 2000 hours

**CONTROL SYSTEM**

DMX channels: 19CH

DMX connector: 3 Pin XLR input and output(hand in hand)

Power connector: PowerCon input and output(hand in hand)

Control mode: master-slave/auto/sound/DMX

Pan: 540º, 16 bits scanning

Tilt: 270º, 16 bits scanning

1 static color wheel: 14 static color gobos+open,with color reposition

1 static gobo wheel: 12 static gobos+open+5 mirror gobos,with gobo reposition and gobo shaking

1 rainbow effect wheel

Prism 1:12 facet rotating prism

Prism 2: 8+16 facet rotating prism

2 prism overlay, motorized focus and frost

Accurate and fast XY axis rotation

Electronic error correction function

Full color TFT LCD color display with 5 buttons

Auto high temperature protection for lamp

**COLOR EFFECT**

Color: 14 colors+open, split color, rainbow effect

Beam angle: 2º

Strobe: 1-25Hz

Linear dimming: 0-100%

Illumination: 200000LUX at 15m

**DIMENSION**

Product dimension(LxWxH): 39\*32\*61CM

Net weight: 20.2KG

SITE DO PRODUTO:

<http://www.sparklaser.com/en/products/207.html>