## 800 BSWF MOVING HEAD

CATEGORIA:

BSW

***CÓDIGO:***

PROFILE 800W

SPL LED 800W

***INFORMAÇÕES:***

800W white LED module with beam angle 4-49°  
Motorized focus,frost filter, zoom, iris, split color, CMY+CTO

2 gobo wheels+1 color wheel + 2 prism  
Smooth cutting disc system

**POWER**  
Input voltage: AC100-240V 50/60Hz  
Power consumption: 900W

**FIXTURE**IP rating: IP20  
Cooling method: fan cooling  
Max ambient temp: 45℃  
Case color: black

**LED**LED: 700W white LED module  
Color Temp:8000K  
CRI:>80  
Average lifespan: 20,000 hours

**CONTROL**DMX channel: 36CH  
DMX connector: 3Pin XLR input/output  
Power connector: PowerCon input  
Control mode: DMX/master-slave/auto/sound/RDM  
Pan: 540º16bits, Tilt: 270º16bits  
Precise and fast Pan/Tilt movements  
Motorized focus, frost, zoom, iris, split color  
3-phase motor for Pan/Tilt, automatic position correction  
Static gobo wheel: 8gobos plus open with gobo shaking function  
Rotating gobo wheel: 7 replaceable gobos plus open with gobo shaking function  
Static color wheel: 6colors plus open,and split color effect  
Smooth CMY+CTO color mixing system  
Prism 1: 3-facet rotating

Aperture: 5-100% smooth adjustment  
Full color LCD touch display with 4 buttons  
With RMD function and software upload via DMX cable  
Cutting disc: a set of controllable light spot cutting angle system composed of  
4 corner cutting pieces, the entire cutting angle system can rotate by 90º, and  
through precise control of the cutting lens, can create any direction of triangle,  
rhombus, rectangle and other shapes of light spots

**COLOR EFFECT**  
Color: 6 colors+open, split color,CMY+CTO color mixing  
Beam angle: 4-49°  
Dimming: 0-100% linear  
Strobe: 0-25Hz, random strobe and pulse strobe  
Lux: 110,000Lux @ 5m & 4°(spot Ø 39mm),

**DIMENSION**  
Product dimension: 50\*34\*80 cm (LxWxH)  
N.W: 40KGS

SITE DO PRODUTO:

http://www.sparklaser.com/en/products/325.html