## 8 - OUTPUT CURTAIN LASER BEAM

CATEGORIA:

LASER

***CÓDIGO:***

SPL G 506

***ESPECIFICAÇÃO:***

8pcs fat beam laser diodes   
Single laser diode control  
7pcs 3W amber LED with beam angle 7°     
Projects strong and sweeping fat beam with 180° TILT, and makes a great and cost effective beam show,  
Applicable for disco, club, KTV, pub, Bar, familiy party etc

***INFORMAÇÕES:***

Power supply:AC 100-240V 50/60Hz

Power consumption:68W

Total Laser power:4W RGB laser

Laser safety:class 4

Laser power/wavelength:8pcs 500mW 638nm  red

Laser safety:class 3B

LED:7\*3W Amber LED (beam angle 7°)

Scan system:stepping motor

Tilt  :180°

Modulation:TTL

Control mode:DMX/Auto/Sound/Master-slave

DMX channel:7/16CH

Display:LED display with 4 buttons

IP rating:IP20

N.W.(KG):6.8KG

G.W.(KG):7.3KG

Product dimension:1000\*84\*173mm

Carton size:122\*36\*25cm (2pcs/carton)

Remarks: other RG,GB,RB,RGB color versions are available too!

SITE DO PRODUTO:

http://www.sparklaser.com/en/products/134.html