## FAT BEAM FULL COLOR LASER MOVING BAR

CATEGORIA:

LASER

***CÓDIGO:***

SPL RGB 508

***INFORMAÇÕES:***

6pcs fat beam laser diodes   
single laser diode control  
semi-conduct laser diode with stable performance and longe liftspan  
sweeping fat beam with Tilt 90° and Pan 240° to make a great and cost effective beam show,  
applicable for disco, club, KTV, pub, Bar etc

Item No:SPL-RGB-508A/SPL-RGB-508

Power supply:AC 100-240V 50/60Hz

Power consumption:150W/200W

Total Laser power:6W RGB laser /1.8W RGB laser

Laser power/wavelength:6pcs 1W intergrated RGB(260mW 638nm red+340mW 520nm green+400mW 445nm blue)

pcs 300mW intergrated RGB(100mW 638nm red+80mW 505nm green+120mW 445nm blue)

Laser safety:class 3B

Pan :90°

Tilt :240°

Control mode:DMX/Auto/Sound/Master-slave

Display:LED display with 4 buttons

IP rating:IP20

N.W.(KG):18.2KG

G.W.(KG):20KG

Product dimension:1000\*146.6\*223.2mm

Carton size:122\*22\*31cm(1pc/carton, G.W:20KG)

SITE DO PRODUTO:

http://www.sparklaser.com/en/products/28.html