## 12\*10W 5in1 PAR LIGHT

CATEGORIA:

PAR LED

***CÓDIGO:***

YG 1203

***INFORMAÇÕES:***

Par light with 12\*10W RGBW UV 5in1 LED  
Beam angle 25º  
IP65 waterproof

****POWER****

Input voltage: AC100-240V 50/60Hz

Power consumption: 150W

****FIXTURE****

IP rating: IP20

Cooling method: convention cooling

Max ambient temp: 45℃

Case color: black

****LED****

LED type:12\*10W 5in1 LED

Average lifespan: 50,000 hours

****CONTROL****

DMX channel: 11/13 DMX channels

DMX connector: 3pin input/output

Control mode: DMX/master-slave/sound/auto

Display: LED display with 4 push buttons

Temperature control for LED

Flicker free operation

****COLOR EFFECT****

Color: RGBW UV

Electronic Dimming: 0-100%

Strobe: 1-23Hz

Beam angle: 25˚

****DIMENSION****

Product dimension: 190x270x95mm

N. W:  1.3 KG

SITE DO PRODUTO:

http://www.sparklaser.com/en/products/241.html