1260 YZ

CATEGORIA:

RIBALTA

***CÓDIGO:***

LED 1260 YZ

***ESPECIFICAÇÃO:***

12\*60W RGBW 4in1 LED

CONTROLE: Single pixel control

MOTOR: Motorized zoom at 3-45°  
Seamless connection between 2units  
Fast movement through high torque motors

***INFORMAÇÕES:***

**Power**

Input voltage:AC100-240V 50/60Hz

Power consumption:680W

Fuse:5A/250V

**Fixture**

IP rating:IP20

Cooling method: fan cool

Max ambient temp:45℃

Case color: black

**LED**

LED SPEC: 12pcs 60W RGBW 4in1 LED

Average lifespan: 50,000 hours

**Control**

DMX channel:18/56CH

DMX connector:3Pin XLR input/output

Power connector: PowerCon input/output

Control mode:DMX/master-slave/auto/sound

TILT:220º

Electronic zoom at 3-45°

LCD color display

fan speed with temperature control

Fan starts working at 45℃, LED intensity drops by 30% when over 70℃.

Daisy chain 8pcs for 220V, 4pcs for 110V at max

**Color effect**

Color: RGBW color mixing

Beam angle: 3-40°

Dimming:0-100%

Strobe:0-25Hz

**Dimension**

Product dimension: 1080\*130\*315 mm

N.W: 22KG

Outer carton size: 116\*21\*42cm

G.W.: 25KG(1pc per carton)

SITE DO PRODUTO:

<http://www.sparklaser.com/en/products/226.html>