## 4 IN 1 B-EYE ZOOM BEAM

CATEGORIA:

WASH

***CÓDIGO:***

SPL LED 640

***INFORMAÇÕES:***

6\*40W RGBW 4in1 LED   
Single pixel control  
Motorized zoom at 3.5-45°  
Seamless connection between 2units  
Fast movement through high torque motors

**LIGHT SOURCES:** 6x 40W 4IN1 RGBW LED  
Beam Angle: 3.5°~ 45°  
Power Consumption: 220W  
Power Voltage: AC 100-240V, 50/60Hz  
Dimension:258mm×178mm×334mm  
Net Weight: 6 Kgs

Carton package 1in1 size: 31\*23\*42cm   Gross weight：7Kgs

Carton package 4in1 size: 65.5\*49.5\*44.5cm  Gross weight：28.5Kgs

**CONTROL**DMX Channel: 21/24/32/56 Channel  
Control Modes: DMX512/Mater-Slave/Auto Run/Music/RDM

**PAN/TILT**Pan/Tilt: 540°/ 270°  
Pan/Tilt Resolution: 8/16 bit

**CONSTRUCTION**Display: LCD Display  
Data In/Out socket: 3-pin XLR sockets  
Power Socket: Powercon in/out  
Protection Rating: IP20

**FEATURES**Motorized liner zoom system, zoom range: 3.5°~45°

Pixels control  
Outstanding color macro effect   
Dimmer: 0~100% smooth dimming   
Variable strobe effects   
Fast, quiet operation and flicker free

SITE DO PRODUTO:

http://www.sparklaser.com/en/products/228.html