## IP65 19\*40W BEE EYE MOVING HEAD

CATEGORIA:

WASH

***CÓDIGO:***

SPL LED 1940 IP

***INFORMAÇÕES:***

19\*40W 4IN1 RGBW LED  
Beam Angle:3.5°- 50°  
Control Modes: DMX512/mater-Slave/Auto Run/Music  
Protection Rating: IP65

**LIGHT SOURCES**

19\*40W 4IN1 RGBW LED

Beam Angle:3.5°- 50°

Power Consumption: 640w

Power Voltage: AC 100-240V, 50/60Hz

Dimension: 434\*532\*298mm

Net Weight:22Kgs

Carton package 1in1 size: 56\*42\*64cm

Gross Weight: 25Kgs

Flight Case 1in2 size: 80\*49.5\*72cm

Gross Weight: 74Kgs

**CONTROL**

DMX Channel:21/23/35/78/92/97/99 Channels

Control Modes: DMX512/mater-Slave/Auto Run/Music

**PAN/TILT**Pan: 540°/ 360°, Tilt: 270°

Pan/Tilt Resolution: 8/16 bit

**CONSTRUCTION**Display:180° reversible 1.8 inch TFT colorful display, Touch Button  
Data In/Out socket: IP65 3-pin / 5-pin XLR sockets  
Power Socket: IP65 Power Con in/out

Protection Rating: IP65

**FEATURES**LED single control, can display arrows, numbers, letters and patterns

High-efficiency optical system, wonderful flower effect plus zoom

Fan work speed auto adjustable with head temperature

Led temperature protection & Fan run speed automatic based on the head temperature.

SITE DO PRODUTO:

http://www.sparklaser.com/en/products/237.html